IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2017-07-04T14:06:45"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Alternate UI 18.0.0.420"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "Hoyt" "Fleming" of Organization (no name given)
  Owner history of Person "Hoyt" "Fleming" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1499128988 (2017-07-04T00:43:08Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING "Fleming Residence" | long name "Fleming Residence" | postal address: "1673 W. Silver Crest"
      IFCBUILDINGSTOREY "First Floor" | long name "First Floor" | elevation 0.
        contains 70 elements
          32 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud" | object type "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud:563555" | names: "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud:569629", "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud:569673", "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud:569810" (+29 more) | material: layers "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud" ("Stucco" 0.0729166666666667, "Plywood, Sheathing" 0.0416666666666667, "Softwood, Lumber" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333) | property sets: Pset_WallCommon
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud" | object type "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud:563399" | names: "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud:571290", "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud:571378", "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud:581774" (+8 more) | material: layers "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud" ("Stucco - Black" 0.0729166666666667, "Plywood, Sheathing" 0.0416666666666667, "Softwood, Lumber" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333) | property sets: Pset_WallCommon
          26 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Interior - 4 3/4" Partition (1-hr)" | object type "Basic Wall:Interior - 4 3/4" Partition (1-hr):1707" | names: "Basic Wall:Interior - 4 3/4" Partition (1-hr):578385", "Basic Wall:Interior - 4 3/4" Partition (1-hr):578455", "Basic Wall:Interior - 4 3/4" Partition (1-hr):578511" (+23 more) | material: layers "Basic Wall:Interior - 4 3/4" Partition (1-hr)" ("Gypsum Wall Board" 0.0520833333333333, "Softwood, Lumber" 0.291666666666667, "Gypsum Wall Board" 0.0520833333333333) | property sets: Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Interior - 6 3/4" Partition (1-hr)" | object type "Basic Wall:Interior - 6 3/4" Partition (1-hr):1710" | names: "Basic Wall:Interior - 6 3/4" Partition (1-hr):579625" | material: layers "Basic Wall:Interior - 6 3/4" Partition (1-hr)" ("Gypsum Wall Board" 0.0520833333333333, "Metal Stud Layer" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333) | property sets: Pset_WallCommon
      IFCBUILDINGSTOREY "Second Floor" | long name "Second Floor" | elevation 12.
        contains 25 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Garage Roof" | object type "Garage Roof" | names: "Garage Roof:Garage Roof:574228" | material: "Default Form" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCROOF | object type "Garage Roof Component:Garage Roof Component:575367" | names: "Garage Roof Component:Garage Roof Component:575369" | parts: 1 IFCSLAB | material: "Default Roof" | property sets: Pset_RoofCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Interior - 4 3/4" Partition (1-hr)" | object type "Basic Wall:Interior - 4 3/4" Partition (1-hr):1707" | names: "Basic Wall:Interior - 4 3/4" Partition (1-hr):593392", "Basic Wall:Interior - 4 3/4" Partition (1-hr):593490", "Basic Wall:Interior - 4 3/4" Partition (1-hr):594292" (+5 more) | material: layers "Basic Wall:Interior - 4 3/4" Partition (1-hr)" ("Gypsum Wall Board" 0.0520833333333333, "Softwood, Lumber" 0.291666666666667, "Gypsum Wall Board" 0.0520833333333333) | property sets: Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:HAF Exterior - Longboard on Wood Stud" | object type "Basic Wall:HAF Exterior - Longboard on Wood Stud:600207" | names: "Basic Wall:HAF Exterior - Longboard on Wood Stud:600514", "Basic Wall:HAF Exterior - Longboard on Wood Stud:600783", "Basic Wall:HAF Exterior - Longboard on Wood Stud:600851" (+2 more) | material: layers "Basic Wall:HAF Exterior - Longboard on Wood Stud" ("HAF Longboard" 0.0729166666666667, "Plywood, Sheathing" 0.0416666666666667, "Softwood, Lumber" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333) | property sets: Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud" | object type "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud:563399" | names: "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud:600784", "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud:600852", "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud:602467" (+2 more) | material: layers "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud" ("Stucco - Black" 0.0729166666666667, "Plywood, Sheathing" 0.0416666666666667, "Softwood, Lumber" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333) | property sets: Pset_WallCommon
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud" | object type "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud:563555" | names: "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud:606282", "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud:606441", "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud:609130" (+2 more) | material: layers "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud" ("Stucco" 0.0729166666666667, "Plywood, Sheathing" 0.0416666666666667, "Softwood, Lumber" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333) | property sets: Pset_WallCommon
      IFCBUILDINGSTOREY "Roof" | long name "Roof" | elevation 24.
        contains 2 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Main Roof" | object type "Main Roof" | names: "Main Roof:Main Roof:574124" | material: "Default Form" | property sets: Pset_BuildingElementProxyCommon
          1 x IFCROOF | object type "Main Roof Component:Main Roof Component:577354" | names: "Main Roof Component:Main Roof Component:577356" | parts: 1 IFCSLAB | material: "Default Roof" | property sets: Pset_RoofCommon

Types
  IFCWALLTYPE "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud" | STANDARD | 37 occurrences | material: layers "Basic Wall:HAF Exterior - Stucco (light) on Wood Stud" ("Stucco" 0.0729166666666667, "Plywood, Sheathing" 0.0416666666666667, "Softwood, Lumber" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333)
  IFCWALLTYPE "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud" | STANDARD | 16 occurrences | material: layers "Basic Wall:HAF Exterior - Stucco (dark) on Wood Stud" ("Stucco - Black" 0.0729166666666667, "Plywood, Sheathing" 0.0416666666666667, "Softwood, Lumber" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333)
  IFCWALLTYPE "Basic Wall:Interior - 4 3/4" Partition (1-hr)" | STANDARD | 34 occurrences | material: layers "Basic Wall:Interior - 4 3/4" Partition (1-hr)" ("Gypsum Wall Board" 0.0520833333333333, "Softwood, Lumber" 0.291666666666667, "Gypsum Wall Board" 0.0520833333333333)
  IFCWALLTYPE "Basic Wall:Interior - 6 3/4" Partition (1-hr)" | STANDARD | 1 occurrence | material: layers "Basic Wall:Interior - 6 3/4" Partition (1-hr)" ("Gypsum Wall Board" 0.0520833333333333, "Metal Stud Layer" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333)
  IFCBUILDINGELEMENTPROXYTYPE "Garage Roof" | 1 occurrence | material: "Default Form"
  IFCWALLTYPE "Basic Wall:HAF Exterior - Longboard on Wood Stud" | STANDARD | 5 occurrences | material: layers "Basic Wall:HAF Exterior - Longboard on Wood Stud" ("HAF Longboard" 0.0729166666666667, "Plywood, Sheathing" 0.0416666666666667, "Softwood, Lumber" 0.458333333333333, "Gypsum Wall Board" 0.0520833333333333)
  IFCBUILDINGELEMENTPROXYTYPE "Main Roof" | 1 occurrence | material: "Default Form"

Property sets
  Pset_WallCommon | properties | on 33 objects (33 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - 4 3/4" Partition (1-hr)" (IFCIDENTIFIER)
    ThermalTransmittance = 1.26633655329166 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 20 objects (20 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "HAF Exterior - Stucco (light) on Wood Stud" (IFCIDENTIFIER)
    ThermalTransmittance = 0.746675918335708 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 17 objects (17 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "HAF Exterior - Stucco (light) on Wood Stud" (IFCIDENTIFIER)
    ThermalTransmittance = 0.746675918335708 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 9 objects (9 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "HAF Exterior - Stucco (dark) on Wood Stud" (IFCIDENTIFIER)
    ThermalTransmittance = 0.746675918335708 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "HAF Exterior - Stucco (dark) on Wood Stud" (IFCIDENTIFIER)
    ThermalTransmittance = 0.746675918335708 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 5 objects (5 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "HAF Exterior - Longboard on Wood Stud" (IFCIDENTIFIER)
    ThermalTransmittance = 0.669519086820665 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - 6 3/4" Partition (1-hr)" (IFCIDENTIFIER)
    ThermalTransmittance = 0.177404167633292 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Interior - 4 3/4" Partition (1-hr)" (IFCIDENTIFIER)
    ThermalTransmittance = 1.26633655329166 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Main Roof" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Garage Roof" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Garage Roof Component" (IFCIDENTIFIER)
    TotalArea = 2288.18044970185 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Main Roof Component" (IFCIDENTIFIER)
    TotalArea = 137.761708586824 (IFCAREAMEASURE) [SQUARE FOOT (conversion based)]
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Garage Roof Component" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Main Roof Component" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 3 (IFCINTEGER)